[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Destination Grouped Networks (C-Web Interface)

You can configure destination networks in grouped format. For JUNOS ASP policies rules, you must enter destination networks in grouped format.

To configure a grouped destination network in a classify-traffic condition:

1. In the side pane, expand a traffic condition, expand Destination Network, and select Group Network.
2. Click Create, enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring Destination Grouped Networks (SRC CLI)
- Configuring Destination Networks (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]