> - Downloads
> - Output Control Keys for monitor Command
> - Related Topics
> - SRC CLI Commands to Monitor Dynamic Service Activator

> ## Output Control Keys for monitor Command

> The output of the monitor command shows how much each field has changed since you started the command or since you cleared the counters by using the c key. For a description of the statistical information provided in the output of this command, see the show command output.

> To control the output of the monitor command while it is running, use the keys listed in Table 1. The keys are not case-sensitive.

> Table 1: Output Control Keys for the monitor Command

> Key | Action
> --- | ---
> c | Clears (returns to zero) the delta counters since the command was started.
> f | Freezes the display, halting the display of updated statistics and delta counters.
> q or Esc | Quits the command and returns to the command prompt.
> t | Thaws the display, resuming the update of the statistics and delta counters.

> #### Published: 2009-09-21

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.