[Contents] [Prev] [Next] [Index] [Report an Error]

# Shutting Down the Device Drivers

To shut down the specified router or device instance:

1. Issue the show sae drivers brief command to view the router or device instances.
2. Issue the request sae shutdown device command to shut down all device drivers.
   - To shut down specific drivers managing a virtual router, use the filter option and specify all or part of the name of the virtual router.
     `
     user@host> request sae shutdown device filter filter
     `
   - To specify that no confirmation is requested before the software shuts down the device drivers, use the force option.
     `
     user@host> request sae shutdown device force
     user@host> request sae shutdown device filter filter force
     `

#### Related Topics

- Shutting Down the Device Drivers (C-Web Interface)
- Viewing Statistics for Device Drivers with the CLI

[Contents] [Prev] [Next] [Index] [Report an Error]