[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Forwarding Class Actions (C-Web Interface)

You can configure forwarding class actions for JUNOS filter policy rules. The forwarding class action causes the router to assign a forwarding class to packets that match the associated classify-traffic condition.

To configure a forwarding class action:

1. In the side pane, select a JUNOS filter policy rule.
2. From the Create new list, select Forwarding Class. Type a name for the action, and click OK.
3. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring Forwarding Class Actions (SRC CLI)
- Configuring Forward Actions (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]