> - Downloads
> - Changing the Number of Requests That the Redirect Server Accepts (C-Web Interface)
> - Related Topics
> - Overview of Traffic Redirection
> - Configuring the Redirect Server (C-Web Interface)

> # Changing the Number of Requests That the Redirect Server Accepts (C-Web Interface)

> If you want to change the number of redirection requests that the redirect server accepts, change the values for the request rates and the client rates.

> To configure the number of redirection requests that the redirect server can accept:

> 1. Click Configure>Redirect Server.

>    The Redirect Server pane appears.

> 2. Change the values in the following boxes as described in the Help text in the main pane:
>    - Request Rate
>    - Request Burst Size
>    - Client Rate
>    - Client Burst Size
> 3. Click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.