> - Downloads
> - Viewing Information About Subscriber Sessions in the Edge Network (C-Web Interface)
> - Related Topics
> - Configuring SRC ACP to Manage the Edge Network (C-Web Interface)
> - Viewing Information About Subscriber Sessions in the Edge Network
> - Viewing Information About Edge Congestion Points by Subscriber Session (C-Web Interface)
> - Viewing Information About Edge Congestion Points by DN (C-Web Interface)

> # Viewing Information About Subscriber Sessions in the Edge Network (C-Web Interface)

> #### Purpose

> View information about subscriber sessions in the edge network with the C-Web interface.

> #### Action

> To view information about subscriber sessions:

> 1. Click ACP>Edge>Subscriber.

>    The Edge/Subscriber pane appears.

> 2. In the Session ID box, enter a full or partial session ID name to display information about one or more specific sessions, or leave this field empty to display information about all sessions.
> 3. In the Slot box, enter the number of the slot for which you want to display subscriber session information.
> 4. Select an output style from the Style list.
> 5. In the Virtual Router Name box, enter a virtual router name to display information about a specific virtual router, or leave the box empty to display information about all virtual routers.
> 6. Click OK.

>    The Edge/Subscriber pane displays a list of current subscriber sessions.

> #### Published: 2009-09-15

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.