> - Downloads
> - Configuring SRC ACP to Manage the Backbone Network (C-Web Interface)
> - Related Topics
> - Configuring SRC ACP (C-Web Interface)
> - Configuring SRC ACP to Manage the Edge Network (C-Web Interface)
> - Configuring SRC ACP to Manage the Backbone Network
> - Configuring Action Congestion Points

> # Configuring SRC ACP to Manage the Backbone Network (C-Web Interface)

> To configure SRC ACP to manage the backbone network:

> 1. Configure network interfaces in the directory.

>    See Configuring Network Interfaces in the Directory .

> 2. (Optional) Configure an action congestion point.

>    See Configuring Action Congestion Points.

> 3. Configure guaranteed bandwidths for services.
> 4. Assign network interfaces to services.

>    See Configuring Congestion Points for Services

> 5. Create congestion points in the directory.

>    See Configuring Congestion Points in the Directory

> 6. Assign interfaces to congestion points.

>    See Assigning Interfaces to Congestion Points

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.