[Contents] [Prev] [Next] [Index] [Report an Error]

# Viewing Routing Table Information

#### Purpose

You can display brief or detailed information about the route from the local system to a remote host.

#### Action

To view brief route information:

`user@host> show route`

    Kernel IP routing table
    Destination     Gateway         Genmask         Flags   MSS Window  irtt Iface
    192.2.2.0  ' '' '' '' '' '*   255.255.255.0       U      0     0      0   eth0
    default         srclab1.mylab.  0.0.0.0           UG     0     0      0   eth0

To view detailed route information:

`user@host> show route detail`

    Kernel IP routing table
    Destination     Gateway         Genmask         Flags Metric Ref    Use Iface MSS   Window irtt
    192.2.2.0  ' '' '' '' '' '*   255.255.255.0       U     0      0     0   eth0 ' '' '0   0     0
    default         srclab1.mylab.  0.0.0.0           UG    0      0     0   eth0 ' '' '0   0     0

The detailed output includes the additional Metric, Ref, and Use fields.

#### Related Topics

- Viewing Information About the Routing Table (C-Web Interface)
- Viewing the Route Information
- Viewing Interface Information
- Testing Connectivity to Remote Hosts
- Overview of Commands to Troubleshoot Connections to Remote Hosts

[Contents] [Prev] [Next] [Index] [Report an Error]