[Contents] [Prev] [Next] [Index] [Report an Error]

# Enabling the Pseudo-RADIUS Authorization Server (SRC CLI)

To enable the pseudo–RADIUS authorization server, configure the pseudo-RADIUS authorization server and make sure the External Subscriber Monitor is running.

To start External Subscriber Monitor:

`

user@host> enable component extsubmon

`

[Contents] [Prev] [Next] [Index] [Report an Error]