> - Downloads
> - Using Map Expressions in Application Protocol Conditions
> - Related Topics
> - Overview of Global and Local Parameters
> - Before You Configure SRC Policies
> - Configuring Application Protocol Conditions (SRC CLI)
> - Configuring Protocol Conditions (SRC CLI)
> - Configuring Protocol Conditions with Ports (SRC CLI)

> ## Using Map Expressions in Application Protocol Conditions

> The application protocol condition is a case in which you might use a map expression to define multiple attributes in one option—the application-protocol option. Maps are a list of attributeName=value pairs separated by commas and enclosed in curly brackets. For example, the map {applicationProtocol=“ ftp” , sourcePort=123, inactivityTimeout=60} supplies the application protocol, source port, and inactivity timeout in one option. “

> Another map {applicationType=“ tcp” , inactivityTimeout=60, destinationPort=80} supplies the protocol, inactivity timeout, and destination port.

> You can also create a local parameter, add a map expression as the default value of the parameter, and then enter the local parameter in the application-protocol option.

> #### Published: 2009-09-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.