> - Downloads
> - Shutting Down the Device Drivers
> - Related Topics
> - Shutting Down the Device Drivers (C-Web Interface)
> - Viewing Statistics for Device Drivers with the CLI

> # Shutting Down the Device Drivers

> To shut down the specified router or device instance:

> 1. Issue the show sae drivers brief command to view the router or device instances.
> 2. Issue the request sae shutdown device command to shut down all device drivers.
>    - To shut down specific drivers managing a virtual router, use the filter option and specify all or part of the name of the virtual router.
>      `
>      user@host> request sae shutdown device filter filter
>      `
>    - To specify that no confirmation is requested before the software shuts down the device drivers, use the force option.
>      `
>      user@host> request sae shutdown device force
>      user@host> request sae shutdown device filter filter force
>      `

> #### Published: 2009-09-15

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.