> - Downloads
> - Viewing Information About SAE Interfaces with the CLI
> - Related Topics
> - Initially Configuring the SAE
> - Reloading Interface Classification Scripts
> - Viewing Information About Interfaces
> - Viewing Information About SAE Device Drivers with the CLI

> # Viewing Information About SAE Interfaces with the CLI

> #### Purpose

> View information about SAE interfaces.

> We recommend that you do not enter the show sae interfaces command without specifying an interface, virtual router, brief, or maximum results to filter the results. Entering the show sae interfaces command can generate a large quantity of results, and processing these results can place a load on the C Series Controller.

> #### Action

> To view information about the router interfaces:

> `user@host> show sae interfaces`
> `
> `

> To view information about particular router interfaces, specify all or part of the interface name.

> `user@host> show sae interfaces interface-name interface-name`
> `
> `

> To view information about interfaces for a particular virtual router, specify all or part of the VR name.

> `user@host> show sae interfaces virtual-router-name virtual-router-name`
> `
> `

> To view only the interface names:

> `user@host> show sae interfaces brief`
> `
> `

> To restrict the number of displayed results:

> `user@host> show sae interfaces maximum-results maximum-results`
> `
> `

> #### Published: 2009-09-10

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.