> - Downloads
> - Creating a Classify-Traffic Condition (SRC CLI)
> - Related Topics
> - Before You Configure Classify-Traffic Conditions
> - Configuring Classify-Traffic Conditions
> - Enabling Expansion of JUNOSe Classify-Traffic Conditions (SRC CLI)
> - Creating a Classify-Traffic Condition (C-Web Interface)
> - Specifying Port Access for Traffic Classification (SRC CLI)

> # Creating a Classify-Traffic Condition (SRC CLI)

> You create classify-traffic conditions within policy rules. Use the following configuration statements to create a classify-traffic condition:

> `
> policies group name list name rule name traffic-condition name {
>   match-direction match-direction ;
>   description description ;
> }
> `

> To add a classify-traffic condition:

> 1. From configuration mode, create a classify-traffic condition inside a policy rule that has already been created and configured. For example, to create a traffic-condition called ctc within policy rule nat:
>    `
>    user@host# edit policies group junos list staticnat rule nat traffic-condition ctc
>    `
> 2. (Optional) For JUNOS ASP policy rules, specify the direction of the packet flow on which you want to match packets.
>    `
>    [edit policies group junos list staticnat rule nat traffic-condition ctc]
>    user@host# set match-direction match-direction
>    `
> 3. (Optional) Provide a description of the classify-traffic condition.
>    `
>    [edit policies group junos list staticnat rule nat traffic-condition ctc]
>    user@host# set description description
>    `
> 4. (Optional) Verify your classify-traffic condition configuration.

>        [edit policies group junos list staticnat rule nat traffic-condition ctc]
>        user@host# show
>        match-direction output;
>        description "Static NAT destination classifier";

> #### Published: 2009-09-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.