> - Downloads
> - Setting Parameter Values for Services (SRC CLI)
> - Related Topics
> - Overview of Services for the SRC Software
> - Setting Parameter Values for Services (C-Web Interface)
> - Enabling the Service Configuration on the SRC CLI
> - Adding a Normal Service (SRC CLI)

> # Setting Parameter Values for Services (SRC CLI)

> Using parameters, you can define general settings in one SRC object and provide specific values for that setting in another object. For example, you can define the general settings for a rate limiter in a policy, insert a parameter for a rate in the policy, and provide specific values for the rate in each service that uses this policy. For information about the concept of parameters, see Parameters and Substitutions .

> Use the following configuration statements to configure parameters for services in the global service scope:

> `
> services global service name parameter {
>   gateway-ip-address gateway-ip-address ;
>   service-ip-address service-ip-address ;
>   service-ip-mask service-ip-mask ;
>   service-port service-port ;
>   substitution [ substitution... ];
>   session-volume-quota session-volume-quota ;
> }
> `

> Use the following configuration statements to configure parameters for services in a service scope:

> `
> services scope name service name parameter {
>   gateway-ip-address gateway-ip-address ;
>   service-ip-address service-ip-address ;
>   service-ip-mask service-ip-mask ;
>   service-port service-port ;
>   substitution [ substitution... ];
>   session-volume-quota session-volume-quota ;
> }
> `

> To configure parameters for services:

> 1. From configuration mode, enter the service parameter configuration. In this sample procedure, the service called Video-Gold is configured in the global service scope.
>    `
>    user@host# edit services global service Video-Gold parameter
>    `
> 2. (Optional) Configure the actual IP address of the gateway router. This value is substituted for the policy global parameter called gateway_ipAddress.
>    `
>    [edit services global service Video-Gold parameter]
>    user@host# set gateway-ip-address gateway-ip-address
>    `
> 3. (Optional) Configure the actual IP address of the host(s) that provides the service. This value is substituted for the policy global parameter called service_ipAddress.
>    `
>    [edit services global service Video-Gold parameter]
>    user@host# set service-ip-address service-ip-address
>    `
> 4. (Optional) Configure the actual IP mask for the service. This value is substituted for the policy global parameter called service_ipMask.
>    `
>    [edit services global service Video-Gold parameter]
>    user@host# set service-ip-mask service-ip-mask
>    `
> 5. (Optional) Configure the actual port for the service. This value is substituted for the policy global parameter called service_port.
>    `
>    [edit services global service Video-Gold parameter]
>    user@host# set service-port service-port
>    `
> 6. (Optional) Configure actual values for other parameters.
>    `
>    [edit services global service Video-Gold parameter]
>    user@host# set substitution [ substitution... ]
>    `
> 7. (Optional) Configure the quota for the volume of data for service sessions. The SRC software uses this value as the default for service sessions created for this service.
>    `
>    [edit services global service Video-Gold parameter]
>    user@host# set session-volume-quota session-volume-quota
>    `
> 8. (Optional) Verify your configuration.

>        [edit services global service Video-Gold parameter]
>        user@host# show
>        service-ip-address 10.10.40.16;
>        service-ip-mask 255.255.255.240;
>        substitution "bw = 5000000";

> #### Published: 2009-09-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.