[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Traffic-Shape Actions (C-Web Interface)

Traffic-shape actions specify the maximum rate of traffic transmitted on an interface. You can create traffic-shape actions in JUNOS shaping policy rules.

To configure a traffic-shape action:

1. In the side pane, select a JUNOS shaping policy rule.
2. From the Create new list, select Traffic Shape. Type a name for the action, and click OK.
3. To create a new value for the Rate parameter, enter a value in the box, and click Add.
4. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring Traffic-Shape Actions (SRC CLI)
- Configuring Traffic-Class Actions (C-Web Interface)
- Configuring Traffic-Mirror Actions (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]