> - Downloads
> - Configuring a C Series Controller to Accept NETCONF Connections (SRC CLI)
> - Related Topics
> - Configuring a C Series Controller to Accept NETCONF Connections (C-Web Interface)
> - Configuring a C Series Controller to Accept SSH Connections (SRC CLI)
> - Configuring a C Series Controller to Accept Telnet Connections (SRC CLI)

> # Configuring a C Series Controller to Accept NETCONF Connections (SRC CLI)

> Use the following configuration statements to enable NETCONF access from the [edit] hierarchy level:

> `
> system services netconf {
>   ssh;
> }
> `

> To configure the C Series Controller to accept NETCONF connections:

> 1. From configuration mode, access the [edit system services netconf] hierarchy level.
>    `
>    [edit]
>    user@host# edit system services netconf
>    `
> 2. (Optional) Enable NETCONF to run over SSH.
>    `
>    [edit system services netconf]
>    user@host# set ssh
>    `

> #### Published: 2009-09-25

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.