[Contents] [Prev] [Next] [Index] [Report an Error]

# Virtual IP Address for Policies

You can configure a virtual IP address to specify an IP address that policies use as a substitution to send traffic to a captive portal.

For information about how to configure a virtual IP address from the SRC CLI, see the documentation for the following statement in the SRC PE CLI Command Reference:

`

shared sae configuration driver {
  virtual-portal-address virtual-portal-address ;
}

`

[Contents] [Prev] [Next] [Index] [Report an Error]