[Contents] [Prev] [Next] [Index] [Report an Error]

## Configuration Statements for Local Configuration

Use the following configuration statements to configure local properties for a component. You enter these statements at various hierarchy levels for different SRC components. This list shows the configuration common to a number of components. For information about configuration specific to a component, such as SAE, NIC, SRC ACP, or SNMP, see the documentation for that component.

`

slot number component-name {
  base-dn base-dn ;
  java-runtime-environment java-runtime-environment ;
  java-heap-size java-heap-size ;
  snmp-agent;
}
slot number component-name initial {
  static-dn static-dn ;
  dynamic-dn dynamic-dn ;
}
slot number component-name initial directory-connection {
  url url ;
  backup-urls [ backup-urls ...];
  principal principal ;
  credentials credentials ;
  protocol (ldaps);
  timeout timeout ;
  check-interval check-interval ;
  blacklist;
  snmp-agent;
}
slot number component-name initial directory-eventing {
  eventing;
  signature-dn signature-dn ;
  polling-interval polling-interval ;
  event-base-dn event-base-dn ;
  dispatcher-pool-size dispatcher-pool-size ;
}

`

For detailed information about each configuration statement, see the SRC PE CLI Command Reference.

#### Related Topics

- Configuring Basic Local Properties
- Local Properties for SRC Components

[Contents] [Prev] [Next] [Index] [Report an Error]