[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Protocol Conditions with Ports (C-Web Interface)

To configure general protocol conditions with ports in a classify-traffic condition:

1. In the side pane, expand a traffic condition, and select Protocol Port Condition.
2. Click Create, enter information as described in the Help text in the main pane, and click Apply.

To configure source and destination ports for protocol conditions:

1. In the side pane, expand Protocol Port Condition>Source Port, and select Port.
2. Click Create, enter information as described in the Help text in the main pane, and click Apply.
3. In the side pane, expand Protocol Port Condition>Destination Port, and select Port.
4. Click Create, enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Configuring Protocol Conditions with Ports (SRC CLI)
- Configuring Protocol Conditions (C-Web Interface)
- Configuring Protocol Conditions with Parameters (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]