> - Downloads
> - Configuring a C Series Controller to Accept Telnet Connections (SRC CLI)
> - Related Topics
> - Configuring a C Series Controller to Accept Telnet Connections (C-Web Interface)
> - Configuring a C Series Controller to Accept SSH Connections (SRC CLI)
> - Configuring a C Series Controller to Accept NETCONF Connections (SRC CLI)
> - Connecting to a Remote Host Through SSH

> # Configuring a C Series Controller to Accept Telnet Connections (SRC CLI)

> You can enable Telnet to let users who have the appropriate privileges connect to a C Series Controller. The system does not allow root access over a Telnet connection.

> Use the following configuration statements to enable Telnet access from the [edit] hierarchy level:

> `
> system services {
>   telnet;
> }
> `

> To configure the C Series Controller to accept Telnet connections:

> `
> [edit]
> user@host# set system services telnet
> `

> #### Published: 2009-09-25

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.