[Contents] [Prev] [Next] [Index] [Report an Error]

## Example: Managing Interfaces by Using the Interface Description

This example causes the SAE to load the DHCP policy group on any interface where the ifAlias starts with DHCP-subscribers.

    [edit shared network device erx-node2 interface-classifier rule rule-2]
    user@host# show
    target /junose/DHCP;
    condition {
      ifAlias=DHCP-subscribers*;
    }

For this approach, you will need to use the ip description command to configure interface aliases that begin with DHCP-subscribers for all interfaces that support DHCP subscribers.

#### Related Topics

- Overview of Configuring Classification Scripts
- Overview of Classification Scripts
- Sending DHCP Options to the JUNOSe Router
- DHCP Options Supported on the SAE

[Contents] [Prev] [Next] [Index] [Report an Error]