> - Downloads
> - Viewing Statistics for Specific Device Drivers with the CLI
> - Related Topics
> - Configuring the Session Store Feature
> - Viewing Information About SAE Device Drivers with the CLI
> - Viewing SNMP Information for Routers and Devices with the CLI
> - Viewing Statistics for Device Drivers with the CLI

> # Viewing Statistics for Specific Device Drivers with the CLI

> #### Purpose

> View statistics for specific router drivers or device drivers.

> #### Action

> To view SNMP statistics for JUNOS router drivers:

> `user@host> show sae statistics device common junos`
> `
> `

> To view SNMP statistics for JUNOSe router drivers:

> `user@host> show sae statistics device common junose-cops`
> `
> `

> To view SNMP statistics for PCMM device drivers:

> `user@host> show sae statistics device common packetcable-cops`
> `
> `

> To view SNMP statistics for third-party device drivers:

> `user@host> show sae statistics device common proxy`
> `
> `

> For example, to view SNMP statistics for JUNOS router drivers:

> `user@host> show sae statistics device common junos`

>     SNMP Statistics
>     Driver type                    JUNOS
>     Number of close requests       0
>     Number of connections accepted 0
>     Number of current connections  0
>     Number of open requests        0
>     Server address                 0.0.0.0
>     Server port                    3333
>     Time since last redirect       0

> #### Published: 2009-09-10

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.