[Contents] [Prev] [Next] [Index] [Report an Error]

## Configuration Statements for NIC Proxies

Use the following configuration statements to configure a NIC proxy for SRC components. You access these statements from the hierarchy for a component, such as:

- [edit shared acp configuration]
- [edit shared sae configuration]
  `
  nic-proxy-configuration name {
  }
  `
  `
  nic-proxy-configuration name resolution {
    resolver-name resolver-name;
    key-type key-type;
    value-type value-type;
    expect-multiple-values;
    constraints constraints;
  }
  `
  `
  nic-proxy-configuration name cache {
    cache-size cache-size;
    cache-cleanup-interval cache-cleanup-interval;
    cache-entry-age cache-entry-age;
  }
  `
  `
  nic-proxy-configuration name nic-host-selection {
    groups groups;
    selection-criteria (roundRobin | randomPick | priorityList);
  }
  `
  `
  nic-proxy-configuration name nic-host-selection blacklisting {
    try-next-system-on-error;
    number-of-retries-before-blacklisting number-of-retries-before-blacklisting;
    blacklist-retry-interval blacklist-retry-interval;
  }
  `

Use the following statements to configure a NIC proxy stub for SRC components. You access these statements from the hierarchy for a component, such as:

- [edit shared dsa configuration]
- [edit shared sae configuration]
  `
  nic-proxy-configuration name test-nic-bindings {
    use-test-bindings;
  }
  `
  `
  nic-proxy-configuration name test-nic-bindings key-values name {
    value;
  }
  `

#### Related Topics

- Before You Configure a NIC Proxy
- For detailed information about each configuration statement, see SRC PE CLI Command Reference.
- Configuring Resolution Information for a NIC Proxy (SRC CLI)
- Changing the Configuration for the NIC Proxy Cache (SRC CLI)
- Configuring a NIC Proxy for NIC Replication (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]