> - Downloads
> - Configuring Traffic-Shape Actions (C-Web Interface)
> - Related Topics
> - Configuring Traffic-Shape Actions (SRC CLI)
> - Configuring Traffic-Class Actions (C-Web Interface)
> - Configuring Traffic-Mirror Actions (C-Web Interface)

> # Configuring Traffic-Shape Actions (C-Web Interface)

> Traffic-shape actions specify the maximum rate of traffic transmitted on an interface. You can create traffic-shape actions in JUNOS shaping policy rules.

> To configure a traffic-shape action:

> 1. In the side pane, select a JUNOS shaping policy rule.
> 2. From the Create new list, select Traffic Shape. Type a name for the action, and click OK.
> 3. To create a new value for the Rate parameter, enter a value in the box, and click Add.
> 4. Enter information as described in the Help text in the main pane, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.