[Contents] [Prev] [Next] [Index] [Report an Error]

# Viewing Statistics for Specific Device Drivers with the CLI

#### Purpose

View statistics for specific router drivers or device drivers.

#### Action

To view SNMP statistics for JUNOS router drivers:

`user@host> show sae statistics device common junos`
`

`

To view SNMP statistics for JUNOSe router drivers:

`user@host> show sae statistics device common junose-cops`
`

`

To view SNMP statistics for PCMM device drivers:

`user@host> show sae statistics device common packetcable-cops`
`

`

To view SNMP statistics for third-party device drivers:

`user@host> show sae statistics device common proxy`
`

`

For example, to view SNMP statistics for JUNOS router drivers:

`user@host> show sae statistics device common junos`

    SNMP Statistics
    Driver type                    JUNOS
    Number of close requests       0
    Number of connections accepted 0
    Number of current connections  0
    Number of open requests        0
    Server address                 0.0.0.0
    Server port                    3333
    Time since last redirect       0

#### Related Topics

- Configuring the Session Store Feature
- Viewing Information About SAE Device Drivers with the CLI
- Viewing SNMP Information for Routers and Devices with the CLI
- Viewing Statistics for Device Drivers with the CLI

[Contents] [Prev] [Next] [Index] [Report an Error]