> - Downloads
> - Configuring the Network Publisher (C-Web Interface)
> - Related Topics
> - Running the Network Publisher
> - Configuring the Network Publisher
> - Troubleshooting Network Publisher Operations
> - Overview of the Network Publisher

> # Configuring the Network Publisher (C-Web Interface)

> Before you configure and run the network publisher, see Before You Configure and Run the Network Publisher.

> To configure the network publisher:

> 1. Click Configure, expand Slot, expand the slot for which you want to configure the network publisher, and then click Network Publisher.
> 2. Under Network Publisher, click Directory.

>    The Directory pane appears.

> 3. In the main pane, review the configuration and make changes as needed.
> 4. Click logger entries, and configure logging as you would for any component.
> 5. Click Routers, and in the Main pane, specify the release number of the JUNOS software.
> 6. Under Routers, click Authentication.

>    The Authentication pane appears.

> 7. Enter authentication properties as described in the Help text in the Main pane, and click Apply.
> 8. Under Routers, click Select.

>    The Select pane appears.

> 9. Define the routing tables and elements in those routing tables from which the network publisher collects information.
> 10. (Optional) Configure a specific router from which the network publisher collects routing table information. The network publisher uses the router-specific properties for specified routers, and applies the general routers properties to all other routers.
>     1. In the Routers pane, select Router in the Create new list.
>     2. Type a name for the new router in the dialog box, and click OK.

>        The router name appears in the side pane and the Routers pane.

>     3. Enter router properties as described in the Help text in the Main pane, and click Apply.
>     4. Under the router, click Authentication.

>        The Authentication pane appears.

>     5. Enter authentication properties as described in the Help text in the Main pane, and click Apply.
>     6. Under the router, click Select.

>        The Select pane appears.

>     7. Define the routing tables and elements in those routing tables from which the network publisher collects information.

> After you configure the network publisher, run it to collect routing table information.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.