[Contents] [Prev] [Next] [Index] [Report an Error]

# Restarting the NIC (SRC CLI)

To restart a NIC host:

- From operational mode, restart the NIC.
  `
  user@host> request restart nic
  `

You can also restart the NIC at the slot level.

#### Related Topics

- Stopping a NIC Host on a C Series Controller (SRC CLI)
- Restarting a NIC Agent (SRC CLI)
- Restarting a NIC Resolver (SRC CLI)
- Changing NIC Configurations (SRC CLI)
- Restarting the NIC (C-Web Interface)

[Contents] [Prev] [Next] [Index] [Report an Error]