> - Downloads
> - Configuring Forwarding Class Actions (SRC CLI)
> - Related Topics
> - Before You Configure SRC Policies
> - Configuring Forward Actions (SRC CLI)
> - Configuring Forwarding Class Actions (C-Web Interface)
> - Parameter Types

> # Configuring Forwarding Class Actions (SRC CLI)

> You can configure forwarding class actions for JUNOS filter policy rules. The forwarding class action causes the router to assign a forwarding class to packets that match the associated classify-traffic condition.

> The type of action that you can create depends on the type of policy rule. See Policy Information Model.

> Use the following configuration statements to configure a forwarding class action:

> `
> policies group name list name rule name forwarding-class name {
>   forwarding-class forwarding-class ;
>   description description ;
> }
> `

> To configure a forwarding class action:

> 1. From configuration mode, enter the forwarding class action configuration. For example, in this procedure, fca is the name of the forwarding class action.
>    `
>    user@host# edit policies group bod list input rule pr forwarding-class fca
>    `
> 2. (Optional) Configure the name of the forwarding class assigned to packets.
>    `
>    [edit policies group bod list input rule pr forwarding-class fca]
>    user@host# set forwarding-class forwarding-class
>    `
> 3. (Optional) Enter a description for the forwarding class action.
>    `
>    [edit policies group bod list input rule pr forwarding-class fca]
>    user@host# set description description
>    `
> 4. (Optional) Verify the forwarding class action configuration.

>        [edit policies group bod list input rule pr forwarding-class fca]
>        user@host# show
>        forwarding-class fc_expedited;
>        description "Expedited forwarding class";

> #### Published: 2009-09-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.