[Contents] [Prev] [Next] [Index] [Report an Error]

## Configuration Statements for SRC CLI Directory Access

Use the following configuration statements to change the connection to the directory that stores SRC configuration information. You enter the system ldap client statement at the [edit] hierarchy level:

`

system ldap client {
  base-dn base-dn ;
  url url ;
  backup-urls backup-urls ;
  authentication-dn authentication-dn ;
  credentials credentials ;
  connect-timeout connect-timeout ;
  time-limit time-limit ;
  eventing;
  polling-interval polling-interval ;
  connection-manager-id connection-manager-id ;
  dispatcher-pool-size dispatcher-pool-size ;
  event-base-dn event-base-dn ;
  signature-dn signature-dn ;
  blacklist;
}

`

| Note: Do not change the value for the enable-eventing, polling-interval, connection-manager-id, dispatcher-pool-size, or event-base-dn statements unless instructed to do so by Juniper Networks. The eventing statement is enabled by default.

#### Related Topics

- Changing Access to the Directory that Stores SRC Configuration Data
- Overview of Configuration for the SRC CLI

[Contents] [Prev] [Next] [Index] [Report an Error]