> - Downloads
> - Configuring Access Control for the VACM
> - Related Topics
> - Configuring the SNMP Agent
> - Configuration Statements for the SNMP Agent

> # Configuring Access Control for the VACM

> To configure the access control for the view-based access control model (VACM):

> 1. Map an SNMPv1 or SNMPv2c community name to a security name.

>    See Associating Security Names with a Community .

> 2. Define a named view.

>    See .

> 3. Map from a group of users or communities to a view.

>    See Defining Access Privileges for an SNMP Group .

> 4. Map a security name into a named group.

>    See .

> #### Published: 2009-09-25

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.