> - Downloads
> - Configuring Next-Hop Actions (SRC CLI)
> - Related Topics
> - Before You Configure SRC Policies
> - Configuring Next-Hop Actions (C-Web Interface)
> - Configuring Next-Interface Actions (SRC CLI)
> - Configuring Next-Rule Actions (SRC CLI)
> - Parameter Types

> # Configuring Next-Hop Actions (SRC CLI)

> Use this action for the ingress side of the interface to specify the next IP address where the classified packets should go. You can configure next-hop actions for JUNOS filters and JUNOSe policy rules.

> The type of action that you can create depends on the type of policy rule. See Policy Information Model.

> Use the following configuration statements to configure the next-hop action.

> `
> policies group name list name rule name next-hop name {
>   next-hop-address next-hop-address ;
>   description description ;
> }
> `

> To configure a next-hop action:

> 1. From configuration mode, enter the next-hop action configuration. For example, in this procedure, nha is the name of the next-hop action.
>    `
>    user@host# edit policies group junose list nexthop-to-ssp rule to-ssp next-hop nha
>    `
> 2. (Optional) Configure the next IP address where the classified packets should go.
>    `
>    [edit policies group junose list nexthop-to-ssp rule to-ssp next-hop nha]
>    user@host# set next-hop-address next-hop-address
>    `
> 3. (Optional) Enter a description for the next-hop action.
>    `
>    [edit policies group junose list nexthop-to-ssp rule to-ssp next-hop nha]
>    user@host# set description description
>    `
> 4. (Optional) Verify the next-hop action configuration.

>        [edit policies group junose list nexthop-to-ssp rule to-ssp next-hop nha]
>        user@host# show
>        next-hop-address virtual_ipAddress;
>        description "Next hop action";

> #### Published: 2009-09-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.