[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Forwarding Class Actions (SRC CLI)

You can configure forwarding class actions for JUNOS filter policy rules. The forwarding class action causes the router to assign a forwarding class to packets that match the associated classify-traffic condition.

The type of action that you can create depends on the type of policy rule. See Policy Information Model.

Use the following configuration statements to configure a forwarding class action:

`

policies group name list name rule name forwarding-class name {
  forwarding-class forwarding-class ;
  description description ;
}

`

To configure a forwarding class action:

1. From configuration mode, enter the forwarding class action configuration. For example, in this procedure, fca is the name of the forwarding class action.
   `
   user@host# edit policies group bod list input rule pr forwarding-class fca
   `
2. (Optional) Configure the name of the forwarding class assigned to packets.
   `
   [edit policies group bod list input rule pr forwarding-class fca]
   user@host# set forwarding-class forwarding-class
   `
3. (Optional) Enter a description for the forwarding class action.
   `
   [edit policies group bod list input rule pr forwarding-class fca]
   user@host# set description description
   `
4. (Optional) Verify the forwarding class action configuration.

       [edit policies group bod list input rule pr forwarding-class fca]
       user@host# show
       forwarding-class fc_expedited;
       description "Expedited forwarding class";

#### Related Topics

- Before You Configure SRC Policies
- Configuring Forward Actions (SRC CLI)
- Configuring Forwarding Class Actions (C-Web Interface)
- Parameter Types

[Contents] [Prev] [Next] [Index] [Report an Error]