[Contents] [Prev] [Next] [Index] [Report an Error]

# Allowing Multiple Logins from the Same IP Address (C-Web Interface)

You can specify whether the SAE allows a login from the same IP address without requiring that the previous session log out first.

- If you enable this setting, the SAE logs in the new subscriber session and automatically logs out the previous session.
- If you disable this setting, the SAE denies login requests if a subscriber session for an IP address is active.

To specify whether the SAE allows a login from the same IP address without requiring that the previous session log out first:

1. Click Configure, expand Shared>SAE, and then click Subscriber Sessions.

   The Subscriber Sessions pane appears.

2. Enable or disable whether the SAE allows a login from the same IP address without requiring that the previous session log out first, as described in the Help text.
3. Click Apply.

[Contents] [Prev] [Next] [Index] [Report an Error]