[Contents] [Prev] [Next] [Index] [Report an Error]

# Before You Configure the NIC

When you use NIC in a client/server configuration, you configure the NIC scenario before you configure the NIC proxies.

Before you configure NIC hosts from the CLI:

- Plan your NIC implementation:
- Choose the NIC configuration scenario to use.

  The default scenario is OnePop.

  For information about NIC configuration scenarios and NIC agents, see Locating Subscriber Management Information.

- Ensure that the appropriate type of router initialization script is configured for the router or network device.

  See Locating Subscriber Management Information.

  Set the editing level for the configuration application you are using, the SRC CLI or the C-Web interface to basic. This ensures that only the statements that you need to configure are visible.

  To set the editing level for the C-Web interface to basic:

  - Click Preferences>Level Basic.

#### Related Topics

- Configuring the NIC (SRC CLI)
- Configuring the NIC (C-Web Interface)
- Starting the NIC (SRC CLI)
- NIC Agents Used in the NIC Configuration Scenarios
- Router Initialization Scripts with NIC Configuration Scenarios
- Verifying Configuration for the NIC (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]