[Contents] [Prev] [Next] [Index] [Report an Error]

# Removing and Installing a Hard Drive

| Note: If your system is powered on, see the SRC PE Getting Started Guide for commands to run before performing these steps.

To remove a hard drive:

1. Slide the locking tab in the bottom-right corner to the right to release the hard drive.
2. Hold the tab to the right and slowly pull the unit out.

To install a hard drive, hold the locking tab to the right and slowly slide the unit into the chassis until it clicks into place.

[Contents] [Prev] [Next] [Index] [Report an Error]