Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Downloads
- CTP2000 4W-EM Interface Connector Pinouts

- Related Topics
- CTP2000 4W&EM Interface Module
- CTP2000 FXS and FXO Interface Module Cables and Pinouts
- CTP2000 Series Console Cable Pinouts

# CTP2000 4W-EM Interface Connector Pinouts

## CTP2000 4W&EM RTM Connector A Pinouts

See Table 1 for connector A pinout information. See CTP2000 4W&EM Interface Module for signal definitions.

Table 1: CTP2000 4W&EM RTM Pinouts–Connector A

Connector A
Pin | Signal | Signal | Pin
--- | --- | --- | ---
1 | Port 0 R | Port 0 T | 26
2 | Port 0 R1 | Port 0 T1 | 27
3 | Port 0 SG | Port 0 E | 28
4 | Port 0 SB | Port 0 M | 29
5 | Port 1 R | Port 1 T | 30
6 | Port 2 R1 | Port 1 T1 | 31
7 | Port 2 SG | Port 1 E | 32
8 | Port 2 SB | Port 1 M | 33
9 | Port 2 R | Port 2 T | 34
10 | Port 2 R1 | Port 2 T1 | 35
11 | Port 2 SG | Port 2 E | 36
12 | Port 2 SB | Port 2M | 37
13 | Port 3 R | Port 3 T | 38
14 | Port 3 R1 | Port 3 T1 | 39
15 | Port 3 SG | Port 3 E | 40
16 | Port 3 SB | Port 3 M | 41
25 | GND | GND | 50

## CTP2000 4W&EM Connector B Pinouts

See Table 2 for connector B pinout information. SeeCTP2000 4W&EM Interface Module for signal definitions.

Table 2: CTP2000 4W&EM RTM Pinouts–Connector B

Connector B
PIN | Signal | Signal | PIN
--- | --- | --- | ---
1 | Port 4 R | Port 4 T | 26
2 | Port 4 R1 | Port 4 T1 | 27
3 | Port 4 SG | Port 4 E | 28
4 | Port 4 SB | Port 4 M | 29
5 | Port 5 R | Port 5 T | 30
6 | Port 5 R1 | Port 5 T1 | 31
7 | Port 5 SG | Port 5 E | 32
8 | Port 5 SB | Port 5 M | 33
9 | Port 6 R | Port 6 T | 34
10 | Port 6 R1 | Port 6 T1 | 35
11 | Port 6 SG | Port 6 E | 36
12 | Port 6 SB | Port 6M | 37
13 | Port 7 R | Port 7 T | 38
14 | Port 7 R1 | Port 7 T1 | 39
15 | Port 7 SG | Port 7 E | 40
16 | Port 7 SB | Port 7 M | 41
25 | GND | GND | 50

#### Published: 2010-05-11