Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Understanding CTPView Network Reports (CTPView)

# Displaying CTPView Network Reports (CTPView)

The CTPView software provides the following reports that detail how ports are provisioned on the CTP platforms in your network:

- Channelization report—Information about all ports on selected CTP platforms.
- Configured port report—Information about only the configured ports on selected CTP platforms.
- Nonconfigured port report—Information about only ports that are incompletely configured on selected CTP platforms.

To display the desired report:

1. In the side pane, select Node > Maintenance.

   The Node Maintenance pane is displayed.

2. Click View Network Host Reports.

   The CTPView Network Reports pane is displayed.

3. Select one or more remote hosts (CTP platform), or click Select All Hosts to select all listed CTP platforms.
4. Click the button for the desired report.

   The report is displayed in the bottom of the pane. Click Clear/Reload Page to remove the report from the pane.

5. (Optional) Click on a column header in the report to sort the data in ascending order for that column.
6. (Optional) Select a different font size for readability.
7. (Optional) Click Printer Friendly Page to display the report in a format suitable for printing.

   You can select and copy the printer-friendly information and paste it in a spreadsheet.

The report database is updated whenever you use the CTPView software to provision a CTP platform. You can also save the CTP platform configuration data to the database automatically or manually.

To update the database automatically, see Configuring Automatic Monitoring of CTP Platforms (CTPView).

1. To update the database manually:
2. In the side pane, select Node > Maintenance.

   The Node Maintenance pane is displayed.

3. Click View Network Host Reports.

   The CTPView Network Reports pane is displayed.

4. Click Update Database.

## Related Documentation

- Understanding CTPView Network Reports (CTPView)

#### Published: 2010-10-05

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out