# Redistributing a Specific IPv6 Static Route Based on the Tag Value

To redistribute a specific IPv6 static route for BGP based on the tag value:

1. Enable an IPv6 instance on the router.
   host1(config)#ipv6
2. Create an IPv6 static route with the tag value as 1234.
   host1(config)#ipv6 route 55::/55 44::44 tag 1234
3. Create a route map and enter into Route Map Configuration mode.
   host1(config)#route-map access
4. Assign a specific tag value to the route map.
   host1(config-route-map)#set tag 1234
5. Exit from Route Map Configuration mode.
   host1(config-route-map)#exit
6. Enter into Router Configuration mode to configure the BGP routing process.
   host1(config)#router bgp 100
7. Configure the IPv6 address family on the BGP router.
   host1 (config-router)#address-family ipv6
8. Configure the route redistribution using the route map.
   host1 (config-router-af)#redistribute static route-map access

#### Related Documentation

- address-family
- ipv6 route
- redistribute
- route-map
- router bgp
- set tag