# Monitoring Static IP Address and MAC Address Pairs Supplied by DHCP Local Server

#### Purpose

Display the static IP address/MAC address pairs that the DHCP local server supplies in standalone mode.

#### Action

To display information about static IP address/MAC address pairs:

    host1#show ip dhcp-local reserved
                              Dhcp Reserved Addresses
                              -----------------------
       Pool        Address                         Hardware
    ----------   ------------   -----------------------------------------------
    cablemodem   10.44.44.100   12-34-12-34-12-34-00-00-00-00-00-00-00-00-00-00
    cablemodem   10.44.44.101   22-33-22-33-22-33-00-00-00-00-00-00-00-00-00-00

#### Meaning

Table 139 lists the show ip dhcp-local reserved command output fields.

Table 139: show ip dhcp-local reserved Output Fields

Field Name | Field Description
--- | ---
Pool | Name of pool in which the address is reserved
Address | IP address that is reserved
Hardware | Address for which the IP address is reserved

#### Related Documentation

- show ip dhcp-local reserved