# ipInterface

#### Description

IP interface

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

None

#### Warning Log

Error status is returned by lower layer configuration; best route is pointing to an unnumbered interface with an invalid source IP address; unnumbered interface is pointing to invalid loopback interface problems; packets received with invalid source IP address on interfaces

#### Notice Log

None

#### Info

None

#### Debug

Interface state transitions and deletions; interface state machine events

#### Filter 1

interface—See description of the ipGeneral interface filter for information about this filter

#### Filter 2

router—See description of the ipGeneral router filter for information about this filter