# Configuring Rate Statistics

To gather rate statistics:

1. Create the statistics profile.
   host1(config)#statistics-profile statpro-5
2. Set the length of time during which statistics are counted.
   host1(config-statistics-profile)#rate-period 45
   Rate period range is 1–43200 seconds.
3. Reference the statistics profile by a QoS profile.
   host1(config)#qos-profile qospro-3 host1(config-qos-profile)#ip queue traffic-class tc1 scheduler-profile sp1 statistics-profile statpro-5
4. Attach the QoS profile to the appropriate interface.
   host1(config)#interface gigabitEthernet 1/0 host1(config-subif)#qos-profile qospro-3 host1(config-subif)#exit
5. (Optional) Display the rate statistics.
   host1#show egress-queue rates interface gigabitEthernet 1/0

#### Related Topics

- Configuring Statistic Profiles for QoS
- Configuring a QoS Profile
- Monitoring QoS Statistics for Rates and Events
- interface
- qos-profile
- queue
- rate-period
- statistics-profile