### JunosE 11.2.0 Release Notes

> ### Resolved Known Problems

> Release 11.2.0 is based on Release 11.1.0 and incorporates all problem resolutions found in that release. The following problems were reported open in Release 11.1.0 and have been resolved in this release, or have been resolved since the 11.1.0 release. For more information about particular resolved problems, you can log in to the JunosE Knowledge Base at https://www2.juniper.net/kb/, enter the defect ID number in the Search by Keyword field, and click Search.

> #### System

> - When you configure, delete, or reconfigure an IPv4 prefix object, the VRRP states and priorities of interfaces of virtual routers are displayed incorrectly in the output of the show ip vrrp command. This problem occurs when both the following conditions are satisfied: [Defect ID 186258]
> - Alternatively enabling and disabling the priority of a virtual router ID from changing in response to the object state change using the ip vrrp track and no ip vrrp track commands
> - The master router also operates as the IP address owner

Copyright © 2010, Juniper Networks, Inc. Report An Error