Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# undebug ip mbgp

#### Syntax

undebug ip mbgp [ in | out ] [ peerAddress [ peerAddressMask ] ]
[ bgpLog ] [ router routerName ] [ filtering-router filteringRouterName ]
[ accessClassName ] [ route-map mapName ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Turns off the display of information previously enabled with the debug ip mbgp command. There is no no version.

#### Options

- in—Displays information for inbound events
- out—Displays information for outbound events
- peerAddress—IP address of BGP peer for which information is displayed
- peerAddressMask—Network mask of BGP peer for which information is displayed
- bgpLog—BGP log of interest; one of the following options:
  - dampening—BGP dampening event; route is suppressed or no longer suppressed by route-flap dampening
  - events—BGP finite state machine events and transitions
  - keepalives—BGP keepalive message events
  - next-hops—BGP next hop events
  - updates—BGP routing table update events
- routerName—Name of the virtual router that owns the BGP router for which information is being displayed
- filteringRouterName—Name of the virtual router that owns the access class and route map parameters
- accessClassName—Name of an access list to filter output
- mapName—Name of a route map to filter output

#### Mode

Privileged Exec

#### Published: 2010-07-14

Help
|
My Account
|
Log Out