# Monitoring AAA Server Attributes

#### Purpose

Display status of the attributes on the AAA server, including AAA accounting duplication and broadcast.

For additional information about the show configuration command, see JunosE System Basics Configuration Guide.

#### Action

To display status of the attributes on the AAA server, including AAA accounting duplication and broadcast:

    host1#show configuration category aaa server-attributes include-defaults
    ! Configuration script being generated on FRI MAY 21 2010 07:52:13 UTC
    ! Juniper Edge Routing Switch ERX1440
    ! Version: 11.2.0 beta-1.1 [BuildId 12073] (April 22, 2010  11:46)
    ! Copyright (c) 1999-2010 Juniper Networks, Inc.  All rights reserved.
    !
    ! Commands displayed are limited to those available at privilege level 15
    !
    ! NOTE:  This script represents only a subset of the full system configuration.
    ! The category displayed is: aaa server-attributes
    !
    virtual-router default
    aaa accounting duplication lac
    aaa accounting broadcast group1
    aaa duplicate-address-check enable
    aaa accounting acct-stop on-aaa-failure enable
    aaa accounting acct-stop on-access-deny disable
    aaa subscriber limit per-vr 0
    aaa intf-desc-format include sub-intf enable
    aaa intf-desc-format include adapter enable
    aaa accounting immediate-update disable
    no aaa ipv6-nd-ra-prefix framed-ipv6-prefix
    no aaa dhcpv6-delegated-prefix delegated-ipv6-prefix
    aaa duplicate-prefix-check disable
    !
    ! ==============================================================================
    !
    virtual-router lac
    no aaa accounting duplication
    no aaa accounting broadcast
    aaa duplicate-address-check enable
    aaa accounting acct-stop on-aaa-failure enable
    aaa accounting acct-stop on-access-deny disable
    aaa subscriber limit per-vr 0
    aaa intf-desc-format include sub-intf enable
    aaa intf-desc-format include adapter enable
    aaa accounting immediate-update disable
    no aaa ipv6-nd-ra-prefix framed-ipv6-prefix
    no aaa dhcpv6-delegated-prefix delegated-ipv6-prefix
    aaa duplicate-prefix-check disable
    !
    ! ==============================================================================
    !
    virtual-router isp
    no aaa accounting duplication
    no aaa accounting broadcast
    aaa duplicate-address-check enable
    aaa accounting acct-stop on-aaa-failure enable
    aaa accounting acct-stop on-access-deny disable
    aaa subscriber limit per-vr 0
    aaa intf-desc-format include sub-intf enable
    aaa intf-desc-format include adapter enable
    aaa accounting immediate-update disable
    no aaa ipv6-nd-ra-prefix framed-ipv6-prefix
    no aaa dhcpv6-delegated-prefix delegated-ipv6-prefix
    aaa duplicate-prefix-check disable

#### Meaning

Table 21 lists the show configuration category aaa server-attributes include-defaults command output fields.

Table 21: show configuration category aaa server-attributes include-defaults Output Fields

Field Name | Field Description
--- | ---
virtual router | Name of the virtual router
aaa accounting duplication | Virtual router used for duplicate accounting
aaa accounting broadcast | Virtual router group used for broadcast accounting
aaa duplicate-address-check | Enabled, disabled
aaa accounting acct-stop on-aaa-failure | Enabled, disabled
aaa accounting acct-stop on-access-deny | Enabled, disabled
aaa subscriber limit per-vr | Enabled, disabled
aaa intf-desc-format include sub-intf | Enabled, disabled
aaa intf-desc-format include adapter | Enabled, disabled
aaa accounting immediate-update | Enabled, disabled
aaa ipv6-nd-ra-prefix framed-ipv6-prefix | Framed-IPv6-Prefix RADIUS attribute used for IPv6 Neighbor Discovery router advertisements
aaa dhcpv6-delegated-prefix delegated-ipv6-prefix | Delegated-IPv6-Prefix RADIUS attribute used for DHCPv6 prefix delegation
aaa duplicate-prefix-check | Enabled, disabled

#### Related Topics

- show configuration category aaa server-attributes include-defaults