Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# neighbor maximum-orf-entries

#### Syntax

neighbor { ipAddress | ipv6Address } maximum-orf-entries maximum

no neighbor { ipAddress | ipv6Address } maximum-orf-entries [ maximum ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
ipv6Address variable added in JunosE Release 8.0.0.

#### Description

Sets the maximum number of ORF entries of a particular type that are accepted from the specified neighbor. The no version restores the default value of no limits.

#### Options

- ipAddress—IP address of BGP neighbor
- ipv6Address—IPv6 address of BGP neighbor
- maximum—Maximum number of ORF entries in the range 0–4294967295; default value is no limit

#### Mode

Address Family Configuration, Router Configuration

#### Published: 2010-07-13

Help
|
My Account
|
Log Out