Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Monitoring the QoS Profiles Attached to an Interface
- Monitoring the QoS Scheduler Hierarchy
- Monitoring Shared Shapers
- node
- qos-interface-set
- qos-interface-superset
- qos-profile
- queue

# Attaching a QoS Profile to an Interface Superset or an Interface Set

You can configure a QoS profile to manage the scheduler resources for an interface set or an interface superset.

Tasks to attach a QoS profile to an interface set or an interface set include:

## Configuring a QoS Profile for an Interface Superset or an Interface Set

To configure a QoS profile to manage the scheduler resources for an interface superset or an interface set:

1. Configure the QoS profile.
   hos1(config)#qos-profile vlan
2. Specify an interface superset or an interface set as a queue.

   For interface supersets:

   host1(config-qos-profile)#superset queue traffic-class video

   For interface sets:

   host1(config-qos-profile)#set queue traffic-class video
3. Specify an interface superset or an interface set as a node.

   For interface supersets:

   host1(config-qos-profile)#superset node scheduler-profile video

   For interface sets:

   host1(config-qos-profile)#set node scheduler-profile video

## Attaching a QoS Profile to an Interface Superset

To attach a QoS profile to an interface superset:

1. Specify the QoS interface superset.
   host1(config)#qos-interface-superset vlan-superset
2. Attach the QoS profile.
   host1(config-qos-interface-superset)#qos-profile business-data

## Attaching a QoS Profile to an Interface Set

To attach a QoS profile to an interface set:

1. Specify the QoS interface set.
   host1(config)#qos-interface-superset vlan-set
2. Attach the QoS profile.
   host1(config-qos-interface-set)#qos-profile business-data

#### Related Topics

- Monitoring the QoS Profiles Attached to an Interface
- Monitoring the QoS Scheduler Hierarchy
- Monitoring Shared Shapers
- node
- qos-interface-set
- qos-interface-superset
- qos-profile
- queue

#### Published: 2010-06-16

Help
|
My Account
|
Log Out