Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Configuring Traffic Classes That Define Service Levels
- Configuring Traffic-Class Groups That Define Service Levels
- Configuring QoS for an L2TP Session

# traffic-class-group

#### Syntax

[ no ] traffic-class-group trafficClassGroupName
[ slot slotNumber | auto-strict-priority | extended ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures a traffic-class group. The no version deletes the selected traffic-class group. You must remove all local (slot-based) instances of a traffic-class group before you can remove the global group.

#### Options

- trafficClassGroupName—Name of the traffic class group; up to 31 characters
- slotNumber—Number of the slot associated with the group, in the range 0—17
- auto-strict-priority—Specifies strict-priority scheduling for the group, regardless of whether the scheduler profile associated with the group node specifies strict-priority scheduling. Only one auto-strict-priority group can exist; this is the default behavior for a group.
- extended—Specifies that strict-priority scheduling for the group is determined by the scheduler profile associated with the group node; scheduling is either hierarchical round-robin or strict priority, but if a strict-priority traffic-class group already exists, this group must scheduled via HRR

#### Mode

Global Configuration

#### Related Topics

- Configuring Traffic Classes That Define Service Levels
- Configuring Traffic-Class Groups That Define Service Levels
- Configuring QoS for an L2TP Session

#### Published: 2010-07-14

Help
|
My Account
|
Log Out