Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# show isis database

#### Syntax

show isis database [ level-1 | level-2 | l1 | l2 | lspid | hostname | detail | verbose ]*
[ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
hostname variable added in JunosE Release 7.3.0.

#### Description

Displays the IS-IS link-state database.

#### Options

- level-1—Displays the IS-IS link-state database for level 1
- level-2—Displays the IS-IS link-state database for level 2
- l1—Displays the IS-IS link-state database for level 1
- l2—Displays the IS-IS link-state database for level 2
- lspid—Link-state PDU identifier in the form xxxx.xxxx.xxxx.yy.zz; when specified, displays the contents of a single link-state PDU by its ID number
- hostname—Displays the IS-IS link-state database for the specified hostname
- detail—Additionally displays contents of each link-state PDU; if not specified, a summary display is provided
- verbose—Additionally displays MPLS traffic engineering information
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Published: 2010-07-14

Help
|
My Account
|
Log Out