Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# set level

#### Syntax

set level atLevel

no set level

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies where to import routes when all of a route map’s match criteria are met. The no version removes the set clause from a route map.

#### Options

- atLevel—Specifies one of the following levels:
  - level-1—Imports routes into a level 1 area
  - level-1-2—Imports routes into a level 1 and a level 2 area
  - level-2—Imports routes into a level 2 subdomain
  - stub-area—Imports routes into an OSPF NSSA area
  - backbone—Imports routes into an OSPF backbone area

#### Mode

Route Map Configuration

#### Published: 2010-07-14

Help
|
My Account
|
Log Out