# Establishing a Static Route

You can set a destination to receive and send traffic by a specific route through the network.

ipv6 route

- Use to establish a static IPv6 route.
- You can set a destination to receive and send traffic from and to a network or to use a specific route through the network.
- Example
  host1(config)#ipv6 route 7fff::0/16 1::1
- Use the no version of this command to remove a static route from the routing table.
- See ipv6 route